|  |
| --- |
| **IMG05 Web House.gif Waikato Building Consents** |
| **Compliance Schedule Details:** **SS 12/1 – Audio Loops** |
| **Please provide the following information with your Building Consent Application and Code Compliance Certificate Application if applicable.** (*If you need help to complete this form, consult the system provider or an IQP who is registered for the system above)* |
| Applicant Name: …………………………………….……..…Site Address: ……………………………………….………….………………………………………………………………..….Existing Compliance Schedule Number(s): *(if applicable)* …………………………………..............................................………………………………….............................................. | Building Name: ………………………………….…………… Installation provider:*(if known)* …………………………….…………………………………............................................Risk / Purpose group: …………………………….………….Fire Hazard Category: ……………………….……………….Total Occupant Load: ……………………….………………. |
| **SPECIFIED SYSTEM DESCRIPTION** (address those items that apply) |
| **Specified systems are:**  | £ Existing £ New £ Modified £ Removed |
| **Type:** |  |
| **Location Plan for specified systems and records is attached**: £ YES £ NO  |
| **No.** |  **Equipment location**  | **Make** *(Main components)* | **Model** |
| 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| 4 |  |  |  |
|  | *If needed continue the list on another sheet of paper* |
| **STANDARDS (**address those items that apply) |
| Specifically, designed solutions do not apply if the system has been installed against a specific Standard(s) / document. |
| **Performance / installation:*****Note:*** *Unless the standard specifies an amendment to the standard, it is to be read as the First Edition (original version).* |  IEC 60118-4:2014+AMD1:2017 CSV Electroacoustics. Hearing aids. Induction-loop systems for hearing aid purposes. System performance requirements. (Original Version – 30 April 2018)£ AS 60118.4-2007 Hearing aids Magnetic field strength in audio-frequency induction loops for hearing aid purposes (Original Version – 20 February 2007)£ AS 1088.4:1987: Hearing Aids. Magnetic Field Strength in Audio-Frequency Induction Loops for Hearing Aid Purposes (Original Version – 01 January 1987)£ BS EN IEC 60118.4:2015+A1:2018 Electroacoustics. Hearing aids. Induction-loop systems for hearing aid purposes. System performance requirements (Original Version – 30 April 2018)£ Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided). £ Other: …………………………………….   |
| **Inspections:*****Note:*** *Unless the standard specifies an amendment to the standard, it is to be read as the First Edition (original version).* |  IEC 60118-4:2014 (Original Version – 30 April 2018)£ AS 60118-4:2007 (Original Version – 20 February 2007)£ Other: …………………………………….  | £ Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided).  *Continue on the next page*  |
| **Maintenance:*****Note:*** *Unless the standard specifies an amendment to the standard, it is to be read as the First Edition (original version).* |  IEC 60118-4:2014 (Original Version – 30 April 2018)£ AS 60118-4:2007 (Original Version – 20 February 2007)£ Other: …………………………………….  | £ Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided).  |
| **INSPECTIONS, MAINTENANCE AND REPORTING** (address those items that apply) |
| **Minimum inspection and maintenance procedures:**  | Regular inspections and planned preventative maintenance and responsive maintenance will be carried out in accordance with the nominated standard/document to ensure continued effective operation of the system during occupation of the building. |
| **Inspection frequency and responsibility:** | Depending on the type of installation and its performance standard/document:£ Specifically, designed solutions: by IQP only.£ Standard /other document: Six-Monthly: by IQP only  |
| **Inspections & Maintenance:***Six Monthly Inspections* | As a minimum, these inspections will include the inspection and testing of:* Magnetic field strength in the specified magnetic field area for the values defined in AS 60118.4
* Magnetic background noise interference from other equipment, where since the last inspection, equipment has been installed, activated or altered in the proximity of the tele loop system. (Such equipment could include electrical fittings, heating systems, electrical controls or equipment, an adjacent loop system or metallic structures).
* Sound amplification installations consisting of loop systems will be tested for sound pressure level and sound distortion. Where room acoustics have been altered since the last inspection, the sound amplification installation will also be tested for spectrum analysis and speech intelligibility. (Room acoustics could have been altered or affected by such things as the addition or removal of carpet, curtains or objects.)
 |
| **Reporting** | The owner will keep records of all inspections, maintenance and repairs undertaken in the previous 24 months. These will be recorded in the On-Site Log Book, which will remain on the premises with the most recent compliance schedule, and as a minimum include:* Details of any inspection, test or preventative maintenance carried out, including dates, works undertaken, faults found, remedies applied and the person who performed the work.
* Form 12A provided annually by the IQP
 |