|  |
| --- |
| **IMG05 Web House.gif Waikato Building Consents** |
| **Compliance Schedule Details:** **SS 15/3 – Fire Separations** |
| **Please provide the following information with your Building Consent Application and Code Compliance Certificate Application if applicable.** (*If you need help to complete this form, consult the system provider or an IQP who is registered for the system above)* |
| Applicant Name: ……………………………………..……..…Site Address: ……………………………………….………….………………………………………………………………..….Existing Compliance Schedule Number(s): *(if applicable)* …………………………………..............................................………………………………….............................................. | Building Name: …………………………………..……………Installation provider:*(if known)* ……………………………………………………………….………………………………….........................................Risk / Purpose group: …………………………….…………..Fire Hazard Category: ……………………….……………….Total Occupant Load: ……………………….……………….. |
| **SPECIFIED SYSTEM DESCRIPTION**  |
| **Specified systems:**  | £ Existing £ New £ Modified £ Removed |
| **Type:** | £ Fire door forming part of a fire separation.£ Walls forming a safe path within a building.£ Fire rated floor in a service cupboard. |
| **Location Plan for exits and records is attached**: £ YES £ NO  |
| **No.** |  **Location**  | **Equipment used** *(e.g. Doors, collars, wraps etc.)* | **FRR** (Fire rating) |
| 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| 4 |  |  |  |
|  | *If needed continue the list on another sheet of paper* |
| **STANDARDS** (address those items that apply) |
| Specifically, designed solutions do not apply if the system has been installed against a specific Standard(s) document. |
| **Performance / installation:** | £ NZS 4520:2010 Fire-resistant doorsets. (Original Version – 29 November 2010) £ AS/NZS 1905.1:1997 Components for the protection of openings in fire-resistant walls - Fire-resistant doorsets. (Original Version – 04 March 1997)£ NZS 4232.1:1988 Performance criteria for fire resisting enclosures - Internal and external fire doorsets. (Amendment 1 – 31 March 1998) £ NZS 4232 Performance criteria for fire resisting closures. Part 2: 1988 Fire resisting glazing systems. (Original Version – 30 May 1988)£ C/AS2 Acceptable Solution for buildings other than Risk Group SH. (Amendment 3 - 02 November 2023) - Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS2 Acceptable Solution for buildings other than Risk Group SH. (Amendment 2 - 05 November 2020) Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS2 Acceptable Solution for Buildings other than Risk Group SH. (Amendment 1 - 27 October 2019). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS2 Acceptable Solution for Buildings other than Risk Group SH. (First Edition - 27 June 2019) Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS2 Acceptable Solution for Buildings with Sleeping (non-institutional) (Risk Group SM). (Amendment 4 - 1 January 2017). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS3 Acceptable Solution for Buildings Where Care or Detention is Provided (Risk Group SI). (Amendment 4 - 1 January 2017). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS4 Acceptable Solution for Buildings with Public Access and Educational Facilities (Risk Group CA) (Amendment 4 - 1 January 2017). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS5 Acceptable Solution for Buildings used for Business, Commercial and Low-Level Storage (Risk Group WB) (Amendment 4 - 1 January 2017). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS6 Acceptable Solution for Buildings used for High Level Storage and Other High-Risk Purposes (Risk Group WS) (Amendment 4 - 1 January 2017). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS7 Acceptable Solution for Buildings Used for Vehicle Storage and Parking (Risk Group VP) (Amendment 4 - 1 January 2017) Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS1 Protection from fire for buildings with sleeping (residential) and outbuildings (risk group SH) (2nd Edition - 02 November 2023). Part 2: Firecells, fire safety systems and fire resistance ratings and Part 4: Control of internal fire and smoke spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 9 - 10 October 2011). Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 8 - 30 June 2010). Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 7 - 1 November 2008). Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 6 - 21 June 2007). Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 5 - 1 October 2005). Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread. £ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 4 - 4 July 2005) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 3 - 25 February 2004) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 2 - 24 April 2003) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Amendment 1 - 6 January 2002) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Errata - 1 July 2001) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS1 Acceptable Solution for Clauses C1-C4 Fire Safety. (Version 1 - 1 June 2001) Part 5: Fire Resistance Ratings and Part 6: Control of Internal Fire and Smoke Spread.£ C/AS3 Acceptable Solution for Clause C3 Spread of fire. (Amendment 4 – 01 January 1997).£ C/AS3 Acceptable Solution for Clause C3 Spread of fire. (Amendment 3 – 01 July 1994).£ C/AS3 Acceptable Solution for Clause C3 Spread of fire. (Amendment 2 – 19 December 2013). £ C/AS3 Acceptable Solution for Clause C3 Spread of fire. (Amendment 1 – (Errata 1) – 15 February 2013)£ C/AS3 Acceptable Solution for Clause C3 Spread of fire. (Original Version – 10 April 2012).. Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided) Other: ……………………………… |
| **Inspections:** | £ AS 1851:2012 Routine service of fire protection systems and equipment (Original Version - 03 December 2012) - Section 12 NZ 4520:2010 Fire resistant doorsets (Original Version - 29 November 2010) - Section 7.£ Signs of damage or deterioration that could adversely affect their fire resistance particularly with respect of closures, exposed fire stopping and surface finish.-No new penetrations without suitable fire stopping-An inspection should carried out to ensure doors forming part of an escape route can be opened and are not, locked, barred, blocked.£ Other: …………………………………… | £ Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided) |
| **Maintenance:** | £ AS 1851:2012 Routine service of fire protection systems and equipment (Original Version - 03 December 2012) - Section 12 NZ 4520:2010 Fire resistant doorsets (Original Version - 29 November 2010) - Section 7.£ AS/NZS 1905:1997 (Original Version - 04 March 1997) - (Doors only)£ Any items found to be faulty are to be rectified as soon as possible. Maintenance will be carried out to ensure fire separation prohibits the spread of fire. New work associated with the fire separation may require a building consent. Maintenance to be constructed by a suitably qualified person.£ Other: …………………………………… | £ Specifically, designed solution prepared by a person who, on the basis of experience and qualifications, is competent to do so. (Details provided) |
| **INSPECTIONS, MAINTENANCE AND REPORTING** (address those items that apply)Regular inspection and responsive maintenance will be carried out to ensure the fire separations prohibit the spread of fire and, in the case of fire doors; occupants are not prevented from leaving the building in the event of an emergency |
| **Minimum inspection and maintenance procedures:**  | Depending on the type of installation and its performance standard/document:£ Specifically, designed solutions: by IQP only.£ Standard /other document: |
| **Inspection frequency and responsibility:** | * + Daily by:
	+ Monthly by:
	+ Six-Monthly by:

Annually by:  |
| £ CS Purpose group£ CL Purpose group£ CO Purpose group£ CM Purpose group£ Building work affecting a Final Exit | £ Owner £ Owner £ Owner IQP only  | £ IQP£ IQP£ IQP  |
| **Buildings requiring daily maintenance:** |  | £ Risk Group CA |
| **Inspections & Maintenance:** |  |
| **Reporting:** |  |